**HENCO Brass heating and sanitary manifolds:** Type VB05, VB06, VB505, VB506

**Manifolds shall comply with EN-ISO 21003-2 and be approved by KIWA, ACS suitable for the following applications:**

1. Drinking Water
2. Heating
3. Other applications (on request and after Henco’s written consent)

The modular self-aligning brass manifolds shall be manufactured from brass CW617N nickel plated and comes with 2, 3 or 4 valves. The manifolds shall be controlled with either a quarter turn or full turn control ABS handle. They shall come in the sizes ¾” or 1” on the supply side, male and female, and outlets with universal Eurocone connections. Manifolds shall have a maximum working pressure of 10 bar between temperatures of -20°C to +95°C.

Manifolds shall be installed and tested following the manufacturer’s installation instructions and according to appropriate codes of practice